## Lower the Vehicle. To lower the vehicle, perform the following:

*Danger notice:* Some standards require that this type of notice *precede* the step in which the danger occurs.

*Format:* notice the following:

* The danger notice is enclosed within a box
* Only the word “DANGER” is all-caps. All-caps for the entire notice would decrease redability.
* The notice is indented to the *text* of the preceding step.
1. Jack up rear of car with a hydraulic jack on a solid part of frame, remove the jack stands, and lower the car to ground.

|  |
| --- |
| **DANGER: Never work underneath a car that is only supported by a jack. Failure to support vehicle may result in death or severe injury if the vehicle falls from the jack.** |

1. Pump the brake pedal until firm.
2. Check that the brake fluid level is between the maximum and minimum lines on the reservoir. Add or remove fluid accordingly.